**User’s Manual**

**Wireless Wi-Fi Adapter**

**Model:** WSNWM600BK/WSNWA600BK

All rights reserved

All information contained in this sheet may not be changed without permission

**CONTENTS**

**[1. Product Information 3](#_Toc427931017)**

[1.1 Product Introduction 3](#_Toc427931018)

**[2. Installation Steps 4](#_Toc427931022)**

**[3. System Connection 7](#_Toc427931023)**

[3.1 Check Device Condition 7](#_Toc427931024)

[3.2 Device Connection 8](#_Toc427931025)

**[4. Home Page Introduction 11](#_Toc427931026)**

**[5. Device Mode Switch 18](#_Toc427931028)**

[5.1 Client+AP Mode 16](#_Toc427931029)

[5.2 AP Mode 16](#_Toc427931030)

1. Product Information

1.1 Product Introduction

Generally speaking, most digital devices in your home are working under 2.4GHz frequency band. Too many devices working in the same frequency band may cause severe interference to make the speed on network become slow, to let you feel bad.**802.11 Wireless Dual Band USB Wi-Fi adapter** can make the choice between 2.4GHz band and 5GHz band become available, can do its auto-negotiation via 802.11 a/b/g/n/ac standard, to let users have the chance to avoid the traffic jam in 2.4GHz band, and use fast 5GHz band to achieve the replacement. This adapter can link to wireless router permitted by 802.11 a/b/g/n/ac specification, for bringing the enhanced network experience, for having faster network speed to users.

**802.11 Wireless Dual Band USB Wi-Fi adapter** selects the latest 802.11 technology. It can reach the wireless transmission speed of 433Mbps at most under 5GHz band, 150Mbps at most under 2.4GHz band and 802.11n pattern. Its auto-negotiation function can adjust work mode and transmission speed automatically when wireless signal interference are detected nearby.

This adapter can use several Wi-Fi encryption pattern, such as WPA, WPA2. This can provide a strong security assurance for users.


It has several work patterns, such as STA pattern and AP pattern. In STA pattern, users can access in wireless router, and in AP pattern, users can share the hotspot and built a network environment to offer a high speed Wi-Fi signal to other devices, just like your PC, laptop, and cell phone.

The dimension of this adapter is mini size, but the contour of it is cool and beautiful. It has a smooth shape and black color but mirror like front look. Our adapters can put the fun in functional and a cool addition to wireless innovation. Just install it, connect it and enjoy it.


2. Installation Steps

Installation steps of adapter driver program is same when it is installed in different operation system. Here takes the steps under Windows 7 for example to explain the installation process.


1. Double click the icon of installation package to start the installation.




2. Choose "I accept the terms of the license agreement" and click "Next".




3. Users can choose the installation type for the actual needs. "Install driver and Mediatek WLAN Utility" is our recommended choice.




4. An UI will pop up to prompt that the system is ready for the installation, then click "Install".



5. The system will show the installation processing bar. After the installation, another interface will show up.



6. When installation process is done, system will remind this information. Click "Finish" will accomplish the installation and log out from installation wizard automatically.



**Notice: If you want to change the installation setup, please click "Back" to return to previous page to set it up again. If you want to quit the installation, please click "Cancel".**


3. System Connection

3.1 Check Device Condition


After finishing the installation, users can find an icon on the task bar, this icon has the information that our product is not existed. Therefore, users need to plug our adapter into the target USB2.0 port.

After plugging in, blue LED indicator on adapter will turn on. At the same time, icon will turn to to inform users that device is available but waiting for connecting.

Users can check its condition in Device Manager.




Double click device name "802.11ac Wireless LAN Card" can check its condition, and the condition will be shown like the below:




Click "OK" can finish this step.

3.2 Device Connection

1. When device is working properly, please double click , or right click it and choose "Lauch Config Utility", users will find an UI like the following picture shows:




2. Click，users can check all available wireless networks:




3. Choose the desired wireless netowrk name, the AP information of that network will be shown at the bottom for reference. Click  will start the connection.


1. If the encryption pattern is NONE, system will start auto-connection, and the basic information of that network will be seen on home page.




1. If the encryption pattern is not NONE, users will enter "Profile Settings" page when click  to connect this wireless network. Authentication pattern and encryption pattern can be revealed in this page.



1. Click  to go to next step to input WPA preshared key.



1. Click  to go to next step. If users input the correct key number, the connection will be done successfully.

Left part is the basic informaton of the connected network. On the right part,  is used to remark the connected one.

4. When the connection is established, LED indicator on device will keep blinking, and users can enjoy the connected network environment.  on task bar is for knowing the connection situation.


**Notice：**

**1. Among the available network selections, 1-14 means the network of 2.4G band, 36-165 means the network of 5G band. If the network is marked as , then it is a 5G network for easy recognization.**

**2. Click  on home page, or right click the related icon on task bar to choose"Exit", network conncetion will be disconnected.**


4. Home Page Introduction

Home page will display some basic information of the connected network, such as SSID, IP address, communication rate, channel, and subnet mask.




We will explain the usage of those functional buttons in the red square frol left to right.

1.  button：This button is for searching all usable wireless networks. By clicking it, a page will show all networks that users can use for check.




Click  can refresh the list information, click  will guide users to "Profile Settings" page for the connection setup of desired network.




Follow and guide and click  to finish the connection setup.

Right click the selected network, users can get the 3 ways of network sequencing. Users can choose the preferred one to sequece the list for convenient check.




Click  can connect to network and enter the page of "Profile Settings"directly.


2.  button：Click this button can gain network link information.




*  button: Showing the link information just like the page above s hows.
*  button: giving some link data information, such like link quality, signal strength, transmit rate and receive rate.




*  button: Providing some data information about some statistic information about transmitting and receiving.




3.  button: Users can enter "Profile List" page by clicking it.




* Click  button, can add a network connection into system, users can refer to chapter 3.2 for detailed information.
* Click  button, can delete the chosen network connection.
* Click  button can do edit operation.
* Click  button, can import some files into system.
* Click  button, can export some files out from system.
* Click  button can add a WPS profile. When finish the related setup, please click  to follow the adding guide and finish it.



4.  button: This button is for advanced setup.



5.  button: This button is for checking product version, MAC address information.




5. Device Mode Switch

Here are 2 extra work modes for users to choose according to their actual needs and real situation: Client+AP mode and AP mode.


Client+AP mode can make device connect WLAN and use itself as a Wi-Fi hotspot simultaneously; AP mode is for access point mode.

5.1 Client+AP Mode

Right click the device icon on task bar, users can see a pop-up list:




Click "Switch to Client+AP Mode", users can see the following page:



Input SSID and pre-shared key and click "OK", then follow the guide to switch the work mode successfully.

5.2 AP Mode

Right click the device icon on task bar, users can see a pop-up list:



Click "Switch to AP Mode", the cofiguration utility will be activitated and the home operation page will pop up.

The device icon will turn to , and the operation method is described in chapter 4.

**Notice: If users want to turn back to client mode, just right click device icon and choose "Switch to Client Mode".**